miim

### Additional Notes

HT400 Jog Box

The SB-Elektronik jog box connects to the SB-Elektronik controller which sends scan codes to PC-DMIS.

SB-Elektronik HT400 Jog Box

No. | SB-Elektronik HT400 Key Function | PC-DMIS Function
1 | Input Control | Insert Move
2 | Input Control (Shift Key) |
3 | Input Control |
4 | Input Control |
5 | Input Control |
6 | Handwheel + Button (Sensor 5) |
7 | Switch the Speed Stages |
8 | Switching between Joystick and Manual Wheel |
9 | Output Stage ON |
10 | End Stage OFF |
11 | Joystick + Button Optional (Sensor 4) |
12 | ON/OFF Axis X |
13 | ON/OFF Axis Y |
14 | ON/OFF Axis Z |
15 | ON/OFF Axis A |
16 | Halve the Set Speed |
17 | Operation Enable for HT |
18 | Accept Restart Point |
19 | Switch the HT Position |
20 | Display the HT Position |
21 | Input Control | Clear / Erase
22 | Input Control | End/Enter
23 | Stop Traversing Record | Hold
24 | Start Traversing Record | Measure
25 | Input Control | Cancel
26 | Display |

Wenzel HT400 Jog Box

The Wenzel HT400 jog box connects directly to the computer through a serial port which then sends scan codes to PC-DMIS.

Wenzel HT400 Jog Box

Wenzel HT400 Key | PC-DMIS Function
X |
Y |
Z |
C |
F1 | End / Enter
F2 | Clear / Erase
F3 | Insert Move
F4 | Measure (or N/A)
F5 | Cancel
F6 |