miim

### Dual Camera Frame Grabber

The dual camera configuration is supported with Matrox and IDS frame grabbers. There is no new registry entry or other such configuration to set in PC-DMIS. PC-DMIS scans for a camera connection on video channel inputs 0 to 3 and assigns them in the order they are found. If cameras are connected to inputs 1 and 3, the PC-DMIS vision probe camera ID will be 0 and 1.

The cameras must be of the same signal type and resolution (ex: NTSC, PAL, etc.)

More:

Connection