core

### Option 2

Manually jog the wrist to the desired AB angles using the jog box. When you reach the desired position, press the Store Move button on the jog box, or take a manual probing. The current AB angles are read automatically. If the A or B angles have changed by more than the PH9 Wrist Warning Delta value available on the Part/Machine tab of the Setup Options dialog box (Edit | Preferences | Setup) then PC-DMIS automatically adds the current AB angles to the Probe Tips list and inserts a TIP/ command in the measurement routine. The new TIP/ command is added to the measurement routine before the stored move or manual probing. When the measurement routine is then executed, PC-DMIS first changes the tip before moving to the programmed location.

For information on the Wrist Warning Delta option, see the "Automatically Adjust Probe Head Wrist" topic in the "Setting your Preferences" chapter.