settingseditor

### AutoShutterTimeToFireStageDrift

This registry entry provides the delay (in milliseconds) that PC-DMIS waits before firing the point detection command when a stage drift has been detected.

This registry entry is only evaluated when the AutoShutterEnable registry entry is set to TRUE (1). If the stage is not stable, then point detection is not reliable.

Entry Name: AutoShutterTimeToFireStageDrift

Entry Type: Whole Number to specify milliseconds. The default value is 2000.