miim

### Interface-Specific Options

ScaleX= Specifies the scale factor for the X-axis.

ScaleY= Specifies the scale factor for the Y-axis.

ScaleZ= Specifies the scale factor for the Z-axis.

MaxSpeed = 400 Sets the maximum speed for the controller. For most controllers, this value is around 400. Some special controllers use a value around 100.

UseSendKey = Defines the function of the Send key. The settings are:

0 - The "Send" key is inactive.

1 - Ends a feature.

2 - Inserts a Move point.

3 - Deletes the last hit taken.

4 - Inserts a manual measured point (hard probe).

UsePButton = 0 Defines the function of the "P" button. The default value is 0 (zero). The settings are:

0 - The "P" button is inactive.

1 - Ends a feature.

2 - Inserts a Move point.

3 - Deletes the last hit taken.

4 - Inserts a manual measured point (hard probe).

ProtoPath = Defines the absolute path to the Proto.exe and CEJComm.ini files. For example: C:\Program Files\CEJ\Proto\.

MapOffsetX = Sets the "X" offset between the CEJ compensation map origin and PC-DMIS probe origin. The software adds the offsets to the probe offsets when the probe data is sent to Proto.

MapOffsetY = Sets the "Y" offset between the CEJ compensation map origin and PC-DMIS probe origin. The software adds the offsets to the probe offsets when the probe data is sent to Proto.

MapOffsetZ = Sets the "Z" offset between the CEJ compensation map origin and PC-DMIS probe origin. The software adds the offsets to the probe offsets when the probe data is sent to Proto.

GeoComp = TRUE Disables the use of Proto geometric compensation when set to FALSE. The default value is TRUE.

TempComp = TRUE Disables the use of Proto temperature compensation when set to FALSE. The default value is TRUE.

MaxControllerMoves = 30 Controls the number of instructions sent to the Proto buffer at a time. The default value is 30.

SendChanging = 0 Disables sending this instruction to Proto when set to 0 (zero). The default value is 0 (zero) but it is usually set to 1. After v1.088 of the Johansson machine interface dll, if the Automatic Probe Changer (APC) is not reported, the software does not send enable or disable probe instructions to the controller.

TimerUpdateInterval = 200 The default value in milliseconds (ms) is 200.

MaxControllerMoves = 30 Sets the count of the controller buffered moves. The default value is 30.

QuitWait = 2000 Defines the time in milliseconds (ms) to wait when quitting after the last command is sent. The default value is 2000.

ResetWait = 400 Defines the time in milliseconds (ms) allowed to the controller after a RESET SOFT and before any other command is sent. The default value is 400.

NoResetOnManStop = FALSE When set to TRUE, the software prevents the RESET SOFT sequence when a stop probe is internally called in manual measure mode. The default value is FALSE.

ForceAPCPresence = TRUE Allows configuration of the SETCONFIG command.

When set to TRUE (default): SETCONFIG n,1

When set to FALSE: SETCONFIG n,0

WaitTimeAfterPhRot = 200 Defines the time allowed in milliseconds (ms) to the controller before sending another command after a probe rotation.