miim

### Updates

Version | Description
1.110 | driver_special_learnmode_option added, with condit. For PC-DMIS v4.2 and later plus error handling for APC PR245311.
1.109 | Handling of error 23 (FOLLOWING [?LAG?]) PR240265.
1.108 | Adjustable time delay after probe rotationWaitAfterPhRotation. The default value is 200 (ms).
1.107 | Anders recommends avoiding HARD reset. All resets sent are now soft resets.
1.106 | PR232281 blocking MANMES/RESET when commands are still executed.
1.105 | Check for PR230553 (no prob noticed) but fixed WaitEnd blocking MANMES when switching to manual mode a after head movement.
1.104 | Check for PR229496 - Send probe pin data executed on each DCC Move or Measure command.
1.103 | PR#228851 + not depending anymore on APC results query. Added ForceAPCPresence in the registry.
1.102 | MANMES sent correctly when switching from DCC mode. NoResetOnManStop registry to avoid numerous resets.
1.101 | Goto manual ignored in change tool check of coordinate system before a measure PR # 223740.
1.100 | VolComp support added as per # 223278.
1.090 | Made sure MANMES is sent after a hit since setting to jog won't for it now #222480.
1.089 | RESET SOFT on Error necessary for Find Hole option #221891
1.088 | PC answer allows or not the send of CHANGE1 / CHANGE0 + #221668. WaitReset time now in the registry.
1.087 | Prehit and Retract now converted from inches! #221567
1.086 | MANMES logic changed #219220
1.085 | Wait for QuitWait ms after bQuitSent received #218600.
1.084 | If CHANGING 0 not allowed, do not send CHANGING 1 either
1.083 | Fixed #218599 and 218600.
1.082 | Internal version.
1.081 | Internal version.
1.080 | Joystick part coordinate system available. #215278.
1.074 | MANUAL/DCC wait reduced. VB offset calculation program added. Needs Proto v2.5.0 release, or later.
1.073 | Internal version.
1.072 | Internal version. Timing issues for PH10 Operation
1.071 | Corrected "PH9 won't reset to 0 at startup!"
1.070 | Buttons can send position, plus better handling of buttons Plus better PH9 error handling (Bug fixes: 215181, 215543, and 215277)
1.060 | Fixed bug 215924 in driver_measure_point.
1.051 | Internal version.
1.050 | Offsets transmitted at the PH9 move, for Proto VolComp.
1.045 | Added map offsets, probe offsets sent real time, and change in MANMES rules of game. Handling of Stop via a reset soft added.
1.044 | INI SETTINGS review, for new registry format.
1.043 | INIT variable (nChanging_0_Enabled) to prevent sending CHANGING 0 (On some controllers!). Added detection of Ruby type for the same reason.
1.042 | Send RESETSCALE if machine type is incremental. Start Proto only if communication fails.
1.041 | In manual mode, set global_commanded_position to last reading.
1.040 | Fixed ACR3 calibration and tool-changers problem after working with Tobias.
1.032 | ResetController better handling. Also, fixed bug for ACR3.
1.031 | Take out LastVector in store_point when in DCC mode (see "CNCMES").
1.030 | Various changes start Proto (location in INI/Registry) by PC-DMIS, user-assignable keys for "p-button" key and "send" key, default TEMPCOMP=TRUE. Fixed bug for improper termination.
1.024 | Better "RESET" handling.
1.021 | Unicode conversion.
1.020 | Communication through Proto.
1.010 | Added VolComp support (with VolCompclass).
1.000 | Initial Release (single-command mode).