laser

#### Boundary Points Area

PC-DMIS lets you define the boundary of a scan. You can do this in these ways:

- Type the XYZ values for the individual boundary points directly

- Measure the points using the laser sensor

- Use the CAD data

Boundary Points and Vectors area

Boundary Points are not available or necessary for Free-form scans

You can change the column widths of the Boundary Point list if you click and drag the right or left edge of a column header to the desired size. The software saves this information to your PC-DMIS Settings Editor each time it changes.

More:

Setting Boundary Points by Typing

Setting Boundary Points Using the Measured Point Method

Setting Boundary Points Using the CAD Data Method

Editing Boundary Points

Clearing Boundary Points

Generate

Undo

Adding and Deleting Boundary Points