miim

#### Miscellaneous

Class9ErrorActions = 0 - Defines what happens when an error of class 9 (Fatal) is received.

Bitmapped:

Bit0

0 = Disable buttons on the ExecuteDialog, except Cancel

1 = Do a Cancel on the execution dialog.

Bit1

2 = Close TCP/IP link to server.This might be useful to prevent recurring messages. Error TCP 10038 will probably show up later.

DelayAfterAbortE = 0.0 - If setting is > 0 , PC-DMIS waits for the setting time (in ms) after sending an AbortE() [PC-DMIS execute dialog button ‘STOP’] before clearing the error. Some servers may send the ACK (&) after receiving an AbortE(), but still not be ready to accept the mandatory following ClearAllErrors().

DroDistance = 0.1 - This sets the machine to move distance triggering a position report. Setting DroTimer and DroDistance to 0.0 will disable I++ DRO Daemon startup.

DroTimer = 5 - This sets the maximum idle time between two position reports, even if the machine doesn’t move. The value must not be less than 0.1.

IgnoreManualRetract = FALSE - When switching to manual mode, the PC-DMIS manual retracts distance is sent to the server. Some servers need it for proper operation, otherwise, the server would use the last sent measure retract. When useless for a server, set to TRUE.

IgnoreWarnings = TRUE - If FALSE, warnings appear as errors. For diagnostic, only.

ManualVectorRuleNumber = 0 - This setting controls the handling of the manual probing IJK vector.

0 - Use server IJK vector values (usually reliable).

1 - Server transmitted IJK is discarded and a vector is calculated from the last DRO values sent by the server before the hit.

2 - No vector is sent to PC-DMIS (unusual).

RetractLimit = 0.0 - Limits the DCC retract after point measure to whatever PC-DMIS is internally computing. Used where the difference between the HM CMMs and I++ retract would make a measurement impossible without a collision (e.g. in square slots). This is a temporary fix and is not useful in versions of PC-DMIS v2011 or earlier.

UseTemperatureCompensationV2 = TRUE - If this Settings Editor registry entry is set to TRUE, you can change the temperature sensors from the I++ registry settings to:

TempSensorX = 3-4

TempSensorY = 5-6

TempSensorZ = 7-8

TempSensorP = 9

For details on the UseTemperatureCompensationV2 registry entry, see the topic "UseTemperatureCompensationV2" in the Settings Editor documentation.