core

Step 7 - Define the Location of the Second Port

In this step for the LSPX5 / HR-XS Probe Changer, you define the location of the second port and all subsequent ports that are available on your probe changer. This message appears:

PC-DMIS Message

From the viewpoint of facing the front of the probe changer, please use the probe tip to take one point on the top of the port, then one point on the external left edge of the port and finally one point on the external front edge of the port for port 2

Prompt to define location of second port

To define the locations of the second port and all subsequent ports, follow the procedure described in step 6.

You have now completed the probe changer calibration process.