core

### OK to Move

(This item exists in the Move Point dialog box, accessible from Insert | Move | Move Point or Operation | Move To.)

If you select the OK to Move check box, PC-DMIS immediately moves the probe to the X, Y, Z position (or by the X,Y,Z increment amount) when you click OK or Create. This allows you to position the CMM without storing the move.

This option fills in the X, Y, Z values with the current position of the probe.