laser

### Laser Plane

Auto Feature dialog box - Plane

To create an auto plane using a laser sensor:

1. Access the Auto Features dialog box (Insert | Feature | Auto), and select Plane.

2. Do one of the following:

- Click on the CAD to give the plane a location and vector. Manually enter any remaining information.

- From the Graphic Display window, use the Laser tab to move the machine to the center of the plane location. Click the Read Point from Position button (). Manually enter any remaining information such as the display, width, length, and other parameters.

- Manually enter the theoretical information for X, Y, Z, I, J, K, display, width, length, and other parameters.

3. Enter the necessary information in the Probe Toolbox tabs. Cycle through the Laser Scan, Laser Filtering, and Laser Clipping properties tabs to enter the information as needed.

4. If desired, click the Test button to test the feature.

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

5. Click Create and then Close.

More:

Plane Specific Parameters

Plane Command Mode Text

Auto Plane Paths