core

### Constructing an Alignment Line

You can construct a line through the current origin, normal to the current workplane. (Input features do not need to be provided.)

To construct an alignment line:

1. Access the Construct Line dialog box (Insert | Feature | Constructed | Line).

2. Select the Alignment option.

3. Do not enter any features.

4. Click the Create button.

The Edit window command line for this option would read:

CONSTR/LINE,ALIGN,length

A - Line through the current origin normal to the current workplane
B - Current workplane
C - Origin

Constructing a line normal to the workplane