miim

## ZEISSTC_RDS

This probe changer is used with the RDS rotating head. It is defined as ZEISSTC_RDS. Calibration for this probe changer is done by taking three hits. With the probe changer running along the X axis at the back of the machine and the user facing the rack the hits will be as follows for each slot:

- On top of the small square at the back right of the slot (0,0,1).

- On the right side of the small square (1,0,0)

- On the back of the small square (0,1,0)

(A) - Hit 1 (Top)

(B) - Hit 2 (Right Side)

(C) - Hit 3 (Back)

The proper INI settings for the RDS tool changer are:

[ZEISS]

TCDepthClearance = -47.360000

TCVerticalClearance = 151.5000

TCLengthClearance = 31.8000

Note that these values were used with older versions of PC-DMIS (for example, version 2.X).