core

Step 10 - Take the Sixth Manual Hit

You will take the sixth manual hit for the HR-MP Probe Changer on the inside left surface of the first port. Once the fifth manual hit is completed, the following message box appears:

PC-DMIS Message

Take a hit on the inside left surface of port 1.

After completing the hit, DCC motion will begin for the rest of the measurement.

1. When you are ready to take the sixth measurement, click OK.

2. Use your machine's jog box to measure the sixth hit on the inside left surface of port 1.

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

3. Click OK. The system goes into DCC mode and measures a series of hits required to accurately locate and orient the rack.

In the next step, you review the calibration results.