laser

### Laser Probe Toolbox: Position Probe tab

Probe Toolbox - Position Probe tab

The Position Probe tab of the Probe Toolbox (View | Other Windows | Probe Toolbox) allows you to select the current probe file and tip and define the current probe location in the active alignment coordinates. You can double click the X, Y, and Z values to edit them.

Warning: When you edit the current probe location, the machine moves to the new coordinate without notice. To avoid injury, stay clear of the laser and the machine. To avoid hardware damage, run the machine at a slower speed.

If you don't see any information in the Probes and Probe Tips lists of the Probe Toolbox, you need to first define a probe. For information on how to define a probe, see the "Defining Hardware" chapter in the PC-DMIS Core documentation.

While you can use this tab with all probe types (contact, laser, and optical), this document only covers PC-DMIS Laser related items. For information about the toolbox as it relates to probes in general, see "Using the Probe Toolbox" in the "Using Other Windows, Editors, and Tools" chapter in the PC-DMIS Core documentation.

More:

To Position Your Laser Sensor

Controls for Position Probe tab