core

Step 8 - Take the Fourth Manual Hit

You will take the fourth manual hit for the HR-MS (used with LSPX1) Probe Changer on the top surface of the left side of the first port.

Once the third manual hit is completed, the following message box appears:

PC-DMIS Message

Take a hit on the top surface of the left side of port 1.
It should be taken near the front.

After completing the hit, DCC motion will begin
for the rest of the measurement.

1. When you are ready to take the fourth measurement, click OK.

2. Use your machine's jog box to take the fourth manual hit on the top surface of the left side of port 1. Take the hit near the front of the port.

WARNING: When you do this, the machine moves. To avoid injury, stay clear of the machine. To avoid hardware damage, run the machine at a slower speed.

3. Click OK. The system goes into DCC mode and measures a series of hits required to accurately locate and orient the rack.

In the next step, you review the calibration results.