settingseditor

### CW43LTTest3AxisSlotTC

Two LED lights in a magnetic relay are located on the back of a three axis slot for a CW43 probe changer: a green light and an amber light. The green light means that the slot relay has power. The amber light is illuminated only if the three axis joint is physically located in the slot.

A True value for this registry entry checks for the amber light, and indicates to the CMM controller that it is safe to apply the 24 volt DC motor power to the three axis joint.

Entry Name: CW43LTTest3AxisSlotTC

Entry Type: True/False value. The default is False.