core

Step 6 - Take the Second Manual Hit

You will take the second manual hit for the LSPX1 Probe Changer in the XY plane on the vertical face in the back of the last port; in this case, port 3. The prompt for the second hit in the back of the last port is:

PC-DMIS Message

Please take a hit in the back of the last port (port 3) directly above the pin.

Prompt for the second manual hit in the back of the last port

1. When you are ready to take the second measurement, click OK.

2. Use your machine's jog box to measure the second hit in the back of the last port as shown below:

View of the second hit in the back of the last port

In the next step, you take the third manual hit.