settingseditor

### CW43LThirdAxisTCLeftToRightLift

Use this registry entry to specify the slot cover lift direction for a CW43 probe changer.

PC-DMIS uses the value for the CW43LThirdAxisTCLeftToRightLift registry entry only when the value for the CW43LThirdAxisTCVerticalSlot registry entry is not set to -1. (A value of -1 means that a three axis slot is not available on the probe changer. This is the default value.)

Entry Name: CW43LThirdAxisTCLeftToRightLift

Entry Type: True or False value. The default is True. To determine the value, stand in front of the probe changer slot and check the slot cover lift direction.

- If the slot cover lift direction is from left to right, set the value to True.

- If the slot cover lift direction is from right to left, set the value to False.