core

Step 3 - Define the Number of Ports

The final step prior to rack calibration is to define the quantity of ports on the rack you are calibrating.

To define the number of ports for your LSPX1 probe changer:

1. Select the Ports tab in the Probe Changer dialog box (Edit | Preferences | Probe Changer):

Probe Changer dialog box - Ports tab

2. In the Active probe changer list, select TYPE=LSPX1.

3. In the Number of ports box, type the number of ports the probe changer has. The number must be a multiple of 3.

4. To save your changes, click Apply.

You are now ready to begin calibration. The next step starts the calibration process.