settingseditor

### DccThicknessIsActual

This registry entry determines how the thickness distance that is provided by the "DccThicknessDistance" is applied.

- 0 - Use the Adjust Theoretical option when the theoretical values need to be adjusted by a thickness because measurements are being done on opposite side of material.

- 1 - Use the Adjust Actual option when measurements are being adjusted by the thickness back to the original theoretical XYZ locations. With this option, it appears that the theoretical and measured values have not been offset and the target is offset. You still need to modify your target so that PC-DMIS drives to the correct location.

- 2 - Use the Adjust None option if you don't need to apply the thickness.

Entry Name: DccThicknessIsActual

Entry Type: Whole Number to specify thickness option. You can type 0, 1, or 2. The default value is 0.