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This document contains an overview of the most important changes per release version. The listed changes can either be new features or bug fixes. A full bug fix list is currently not available.
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[bookmark: _Toc238222953][bookmark: _Toc240632671]18.09.2026: no new version

[bookmark: _Toc240632672]11.09.2026: Build 10.32327

[bookmark: _Toc240632673]04.09.2026: Build 10.32327
[bookmark: _Toc240632674]Interfaces
· Leitz: expansion coefficient was send in wrong unit when activating workpiece temperature compensation
[bookmark: _Toc240632675]CHECK-Jobs
· Unlocking the laser during the measurement lead to error in ISO 10360 job.

[bookmark: _Toc240632676]28.08.2026: Build 9.32316
[bookmark: _Toc240632677]General
· Measurement settings: do not allow start of recording to be larger than the measurement time
[bookmark: _Toc240632678]CAL-Jobs
· Rotary axes: make sure plots have axes steps displayed also for small measurement ranges
[bookmark: _Toc240632679]CHECK-Jobs
· Reassigning machine with different volume: 
· only allow this in case volume fits the setup
· check existing lines for fitting into the volume. If this is not the case the actions will be deleted and have to be recreated by measuring the laser position again.
[bookmark: _Toc240632680]Errormaps
· Heidenhain: calculation of location errors into component errors was incorrect for XZY kinematic

[bookmark: _Toc240632681]21.08.2026: Build 8.32279
[bookmark: _Toc238222954][bookmark: _Toc240632682]General
· Reload measurement data:
· Show proper messages and explanations why reloaded data has been discarded.
[bookmark: _Toc240632683]Interfaces
· Maestro:
· Added missing OnTheFly settings for measurement settings.

[bookmark: _Toc240632684]14.08.2026: Build 7.32270
[bookmark: _Toc240632685]Interfaces
· Laser Tracer:
· Added button in LT3Man for resetting the system.
· Increased timeout to 90s when waiting for TracMan to launch.
[bookmark: _Toc240632686]CAL-Jobs
· Job settings GUI:
· Machine volume limits validation failed when there were more than 2 decimal places.
· Number of steps was not properly updated when using the buttons for adjusting the step sizes and shifting the machine volume.

[bookmark: _Toc240632687]07.08.2026: Build 6.32241
[bookmark: _Toc240632688]General
· CNC Generator: Dwell time for linear axis was still displayed when unselected when rotary axes were involved 
[bookmark: _Toc240632689]Interfaces
· Maestro: Copying compensation data file to the controller failed
[bookmark: _Toc240632690]CAL-Jobs
· Results window: Measured points in the 3D plot changed colors when selected 

[bookmark: _Toc240632691]31.07.2026: Build 5.32207
[bookmark: _Toc240632692]CHECK-Jobs
· Non measurable actions were not deleted after job setting had been changed accordingly

[bookmark: _Toc240632693]24.07.2026: Build 4.32187
[bookmark: _Toc240632694]General
· Laser position measurement settings window: performance issues when using window with machine not being connected
[bookmark: _Toc240632695]Interfaces
· Lasertracer, EDS: 
· wired temperature sensor sporadically gave the error message, that no valid data could be acquired due to low signal.
· Thresholds for signal and battery adapted due to messages that signal or battery were too low although sensor was still working with those values
· Leitz: error message that no probe data could be read from the controller sporadically appeared during measurements
[bookmark: _Toc240632696]CAL-Jobs
· Start measurement window: path preview did not work correctly when measuring short path at the same time

[bookmark: _Toc240632697]17.07.2026: Build 3.32167
[bookmark: _Toc240632698]General
· Logging: make sure time stamps are identically generated in all log files
· Reports: images were not always displayed correctly and on the correct page
[bookmark: _Toc240632699]Interfaces
· Load and connect did not work in all cases, license was sometimes still blocked
· LT3Man: after refresh, the Bluetooth symbol was greyed out although remote was still connected
[bookmark: _Toc240632700]Errormaps
· Fagor: added output for HAM errors, even if they were not calculated
[bookmark: _Toc240632701]CAL-Jobs
· Adjust reflector: window did not open 
· Planning window, adaptive box usage: changes were not displayed correctly when editing frame settings directly after the window appears
· Short program measurement was not stopped in case laser locked out
[bookmark: _Toc240632702]CHECK-Jobs
· Position measurement settings, mirror measurement: when moving machine to center of cross, the distance from center of cross was automatically set higher than 100 mm.

[bookmark: _Toc240632703]10.07.2026: Build 2.32139
[bookmark: _Toc240632704]Errormaps
· Siemens VCS, rotary axes: grid points had wrong unit
· Siemens MEC, settings window: some edit fields were cut of with large font size selected
[bookmark: _Toc240632705]Interfaces
· Etalon Lasertracer: measurement could be started although laser was not completely initialized yet
[bookmark: _Toc240632706]CAL-Jobs
· Linear axes, planning window: 
· sometimes not all planned positions were displayed although option to show all positions was selected
· Inclination was sometimes calculated with one step size missing, so that min/max elevation was still not valid

[bookmark: _Toc240632707]03.07.2026: Build 1.32098
[bookmark: _Toc240632708]General
·  Licenses for metrology devices were sometimes randomly blocked

[bookmark: _Toc240632709]26.06.2026: Build 0.32041
[bookmark: _Toc240632710]CAL-Jobs
· Switching between static and OnTheFly measurement after measurements had already been carried out deleted measured data. Switching this option now is no longer allowed after measurements have been carried out

[bookmark: _Toc240632711]19.06.2026: Build 0.32032
[bookmark: _Toc240632712]General
· When starting a measurement, the information shown when hovering over the play button was not always shown in the selected language.
· Addign a picture for a machine via Drag and Drop was no longer accessible 
[bookmark: _Toc240632713]Interfaces
· Etalon Lasertracer: beam break was not reset correctly when starting check line measurements
[bookmark: _Toc240632714]CAL-Jobs
· Compare errormaps report did show wrong and mixed up positions in the plots

[bookmark: _Toc240632715]12.06.2026: Build 0.31986
[bookmark: _Toc240632716]Interfaces
· Siemens: reworked check of actual position versus planned target position, sometimes a wrong position with an offset of 360° was written into the measurement data file (e.g. 330 instead of -30)
· Heidenhain:
· Linear axes online, measurement in TRP: measurement was not starting anymore
· Rotary axes online: feed in CNC program had the wrong unit
[bookmark: _Toc240632717]CAL-Jobs
· Rotary axes planning was sometimes not updating anymore

[bookmark: _Toc240632718]05.06.2026: no new version
[bookmark: _Toc240632719]General
· When measuring the same position or line several times without closing the measurement window, only the last measurement was displayed in the application
· Support and about window was never displayed with English language enties
· Measurement window did show too many temperature warnings, now one warning is displayed and the next message will give the information that temperatures are measured again
[bookmark: _Toc240632720]Interfaces
· Etalon Lasertracer: LT3Man had the wrong version number

[bookmark: _Toc240632721]29.05.2026: Build 0.31891
[bookmark: _Toc240632722]General
· Fixed software crashes when using integrated EDS with metrology device
· When copying a machine and assigning it to the same job as the original machine, the step size for the X axis changes while step sizes for the Y and Z axes remained unchanged
[bookmark: _Toc240632723]Interfaces
· Etalon Lasertracer:
· integrated EDS randomly disconnected itself
· Installation of LT3Man now has separate desktop icon
· Fixed error in Bluetooth remote assignment
[bookmark: _Toc240632724]CAL-Jobs
· Settings window, volumes: identifiers for measuring volume start and end were not labeled consistently

[bookmark: _Toc240632725]22.05.2026: Build 0.31894
[bookmark: _Toc240632726]Interfaces
· Etalon Lasertracer: Language in LT3Man was not correctly set in all windows after changing language in Unical
· Simulated LaserTRACER-NG interface now adds random noise to measured lengths

[bookmark: _Toc240632727]18.05.2026: Build 0.31858
[bookmark: _Toc240632728]General
· Meaurement window: added observers for air humidity and air pressure
· Machine command action window: text was outside the box when it got longer
· Measurement, maximum length error exceeded: show warning besides setting observer field from green to red
[bookmark: _Toc240632729]Interfaces
· Leitz: fixed error when reading probe offset while starting the measurement
[bookmark: _Toc240632730]CHECK-Jobs
· Text layover for certain plots and their legends

[bookmark: _Toc240632731]08.05.2026: Build 0.31842
[bookmark: _Toc240632732]CAL-Jobs
· Rotary axes: improved planning for table axes
[bookmark: _Toc240632733]CHECK-Jobs
· Integrated display of cosine errors for measured lines
· Integrated special Zeiss Report with corresponding license
[bookmark: _Toc240632734]Interfaces
· Reworked Siemens Online interface (still beta)
· Reworked Heidenhain Online interface (still Beta)
· Interface to new Etalon Lasertracer (Beta)
· Reworked Hexagon Common Control interface
· Added interface monitor window for CMM interfaces
[bookmark: _Toc240632735]Compensation formats
· Integrated Fidia volumetric compensation format
· Integrated Fidia SEC compensation format
· Integrated Siemens MEC format (Beta)
· Integrated Fagor volumetric compensation format
· Integrated Mazak volumetric compensation format
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