#### Normal Feature - Type2

This label type requires the selection of Features. If the Feature Variable list is displayed in the side bar, this chart icon will be grayed out. Access the Feature list in the side bar, and apply some features to the CAD tab to display this label.

The Normal Feature - Type2 label type updates the labels in the CAD tab to display a table-like chart with multiple rows and columns. The first row is a single cell with the feature's ID. The second row is a header indicating what is displayed in the remaining rows, in this case, plus and minus tolerance values and the deviation.

Rows three through five display the tolerance and deviation values for only the X, Y, and Z axes of the feature:

Zoomed in view of the CAD tab showing the Normal Feature - Type2 label type

You can use the Label Content area of the Label Settings dialog box to change what statistic value is displayed. See "Label Settings".

You can use the Feature Label Settings dialog box to colorize only critical axes. See "Feature Label Settings".