###

### Configuring Hardware and Connections

These items appear on the Config tab of the ribbon. Both the administrator and the operator may access them.

Open RS-232

The Open RS-232 button in the Port group makes the RS-232 port available for communication between the DataGauge+ application and the connected device.

Close RS-232

The Close RS-232 button in the Port group closes the RS-232 port so that no communication is available between the DataGauge+ application and any connected devices.

Communication

The Communication button in the Configure group starts the DataGauge+ Communication Config Wizard. See "Communication Configuration Wizard" for more information

Channel

The Channel button in the Configure group displays the Channel Selection dialog. See "Channel Selection" for more information.

Select the Setup button to display the DataGauge+ Devices Configuration Wizard. See "Devices Configuration Wizard" for more information.

More

Communication Config Wizard

Channel Selection

Devices Configuration Wizard