### Using the List View Mode

This simple view mode shows the feature names followed by the reported axis:

The List View Mode

The following colors are used by default:

- Red - Out of tolerance

- Yellow - Out of control

- Fuchsia - Out of tolerance and out of control.

- Dark yellow - Failed an AT&T test.

- Green - Good

Out of tolerance variables will flash on and off.

More:

Working with Alarms and Control Limits