### Leader Line End Location

The Leader Line End Location tab inside the Data Editor tab lets you view and manage all the X, Y, and Z end location coordinates for features' leader lines when those features are applied to the CAD tab.

When you access the Leader Line End Location tab, you may not see anything. As with the other tabs in the main view, you need to first apply data to this tab. Once data is applied, each feature appears listed in a table-like view:

Some sample rows in the Leader Line End Location tab

From left to right, the first column displays all the feature names. The second column shows the alignments each feature is based on. If there is no alignment, the cell is empty. The remaining columns show the X, Y, and Z values for each feature's leader line end point.

These procedures provide specific information on things you can do with leader line end locations:

- Editing Leader Line End Locations

- Restoring Leader Line End Locations to Their Original Values

- Importing Updated Leader Line End Locations

- Exporting Leader Line End Locations