#### Exporting Leader Line End Locations

You can export leader line end locations from a PC-DMIS part program by choosing File | Export | Generic File from the PC-DMIS menu structure and from Output Type choosing Feature. This generates a text file that can then be imported into DataPage+.

You can also manually create a text file. If you do, the text file need to be formatted so that all data (feature or location names; X, Y, and Z location values; and any I, J, or K direction values) are separated by a space character, like this:

<feature name> <x> <y> <z>

<location name> <x> <y> <z>

<feature name> <x> <y> <z> <i> <j> <k>

<location name><x> <y> <z> <i> <j> <k>

For example the following when imported would update the leader line end location for CIR1:

CIR1 93 75 0

Leader line end locations can only be imported for existing features.