#### Measurement Deviation Chart

The Measurement Deviation Chart displays deviation trends in incoming measurement data without needing to generate any reports. The chart displays a vertical colored bar. A longer colored bar means a greater deviation from the nominal. The two solid orange lines mark the locations of the caution limit at -75% and +75%.

- Red indicates those variables that are out of tolerance

- Yellow indicates those variables that are between 75% and 100% of specification limits.

- Green indicates those variables that are within 75% of specification limits.

Sample Chart