#### Device Wizard

Use this wizard to set the device name, channels and its commands.

1. Login as an administrator.

2. On the Configure tab, in the Communication group, click Device Management to display the Device Management dialog box.

Device Management dialog box

3. To open a Device Wizard, right-click anywhere in the dialog box, and click Add.

Device Wizard - Device Name Screen

4. In the Device Name box, type a name for the device.

5. Click Next to advance to the next screen.

6. In the Channels box, type the number of channels used by your device.

Device Wizard - Number of Channels screen

7. Click Next to advance to the next screen. In the Communication Commands screen, type the communication commands in the boxes to connect to the device.

Device Wizard - Communication Commands screen

In the Commands area, in the individual boxes, type the specific commands provided by the device manufacturer to connect to the device, initialize the device, open a channel, receive measured values, and then to close a channel.

Connection Confirmation Command - Type a desired string to verify the device is connected.

Device Initialization Commands - Type a string to initialize the device.

Open Channel Command - Type a string to pick up the data from different hand gauge.

Close Channel Command - Type a string to close the communication with channel.

Get Measured Value Command - Type a string to manually get data from the hand gauge through a specific command.

Use the Regex area to type a regular expression provided by the device manufacturer to verify that a connection has been established and to extract measured data from the string of characters returned from the device.

Connection Verification Regex - Type an expression to verify that a connection has been properly established with the device.

Measured Value Query Regex - Type an expression to locate the measured value contained within a string sent by the device following measurement.

8. Click Back at any time to return to the previous screen.

9. Once you are done filling out the Wizard, click Finish to store the updates and return to the DataGauge+ screen. Click Cancel to exit the wizard without saving your changes.