### Feature Label Settings

From the CAD tab, select Options and then Feature Label Settings... to access the Label Settings dialog box. This menu item is only available if you've selected Feature from the side bar and applied features to the CAD tab. See "Selecting and Applying Features or Feature Variables".

Feature Label Settings dialog box

This dialog box determines whether or not normal feature type labels colorize all axes or just critical axes according to the color bar when drawn in the CAD tab.

Show Color By Color Bar

For all axes - This shows the color for all axes according to the color bar.

For critical axes - This shows only the critical axis (or axes) according to the color bar. Non-critical axes are shown in black.

Input critical axes - This box lets you define the critical axes. Type the axis or axes into this box. If defining multiple axes, separate each typed axis with a space character.

For example, consider the following:

Sample Normal Feature - Type1 label with all axes shown according to the color bar

Sample Normal Feature - Type1 label displaying only the critical T axis