### fHα

fHα is a symbol used by your gear standard. It specifies the distance between two design profiles which intersect the mean profile at the end points of the evaluation range. The profile angle deviation is positive when the mean profile rises from the design profile towards the nonmaterial side at the tooth tip; it is negative when the mean profile drops towards the material side at the tooth tip. Please see the appropriate gear standard for a detailed definition of this value.