## Analyzing a Bevel Gear

The Analyze dialog box allows you to define parameters and provide report information for analysis reports. Once you complete the gear measurement, you can use this dialog box to produce a graphical report of the measurement (see the sample reports below).

| Clicking the Analyze button or selecting the Measure | Analyze menu option displays the Analyze dialog box.

Analyze dialog box

Analysis Options Area

For each of the analysis options, measured data must exist in order to select the option for inclusion in the report.

Topopragh: Select this option for Topography output to be created. Click Parameters to make changes to the Topography Parameters. See "Defining Topography Data".

Pitch Runout: Select this option for Pitch/Runout output to be created. Click Parameters to make changes to the Pitch/Runout Parameters. See "Defining Pitch/Runout Data".

Plot Information Area

This area allows you to include general purpose information appear in your analysis report, such as: Program Number, Serial Number, Inspector, Machine ID, Date/Time, Drawing No., Part/Mach No. and Notation. This information will be included in the header of your report. The Date/Time value is supplied automatically based on the time of gear measurement.

Clicking this button creates the report based on the different options and values set in the Analysis Setup dialog box. It sends the report to the output device specified in the Display option. Measured data is spooled to the Quindos PageViewer application where you can view and print your report(s). See "Appendix A: Using Quindos PageViewer".

Clicking this button closes the Analysis Setup dialog box.

Important! Quindos PageViewer depends on PC-DMIS Gear being open. If you close PC-DMIS Gear, Quindos PageViewer and any open analysis reports will also close.

See the "Sample Pitch & Runout Report" and "Sample Topography Report" topic for examples of the bevel gear reports that are created by PC-DMIS Gear.

More...

Sample_Pitch_&_Runout_Report

Sample_Topography_Report