## Step 10: Evaluate the Gear

When the gear measurement is complete, PC-DMIS Gear can evaluate the measurement results according to the specified standard, and generate reports and plots.

To evaluate the gear measurement:

1. Select the Operation | Evaluate Gear… menu option or the Evaluate toolbar icon…

…to open the Evaluate Gear dialog box. The available options and plot information will vary depending on the type of gear that you are defining.

2. For detailed information about evaluating the gear, refer to one of the following:

1. - Cylinder gear: See "Evaluating a Cylinder Gear".

   - Bevel gear: See "Evaluating a Bevel Gear".

When you click the OK button, the measurement data appears in the Gear Report window, where you can view and print your report(s). See "Using the Gear Report Window".

Important! The Gear Report window can be viewed only when PC-DMIS Gear is open. If you close PC-DMIS Gear, the Gear Report window, along with all open evaluation reports, will close.

Step 11: Review Measured Data...