### Runout

The Runout value can be determined theoretically by placing balls of a specified diameter into the gaps of each tooth. The center points of all spheres will form a circle. This circle is compared to the pitch diameter circle where the difference between the largest radius and the smallest radius is considered to be the runout value. Consult your gear standard for a detailed definition of this term.