## Step 2: Launch PC-DMIS Gear

To launch PC-DMIS Gear:

1. Ensure that the Gear and/or Spiral Bevel Gear option is enabled on your portlock.

Note: If neither option is enabled on your portlock, PC-DMIS Gear installation will be blocked and an error message will appear. If only one option is enabled on your portlock, then only that module will be available in PC-DMIS Gear.

2. Select Start | PC-DMIS GEAR, or double-click the PC-DMIS Gear shortcut icon on your desktop:

3. The PC-DMIS Gear application appears. If this is the first time the application is run, it will start in Programmer Mode:

PC-DMIS Gear – Programmer Mode

Step 3: Modify PC-DMIS Gear Settings...