### Step 4: Selecting a Probe

The Select Probe screen lets you choose what probe should measure your part.

Access the Select Probe screen by pressing the following sequence of soft keys from the main screen:

- Press the Probe soft key.

- Press the Select a Probe soft key. The Select Probe screen then appears.

Select your probe you want to use from the Probe area, and then press the Confirm and Append Current Command to End soft key.

NC Gage will insert the probe into the part program's tree view.

Available Navigation Bar Soft Keys on this Screen:

| Backward When enabled, this soft key scrolls back to any additional buttons available on the first page for this screen. |  | Select a Probe If the Select Probe screen isn't the current screen then this soft key accesses the Select Probe screen. If the Select Probe screen is already visible then this soft key selects scrolls through each probe in the Probe list with each touch of the soft key.
| Create a New Probe This soft key lets you create a new probe by accessing the Create New Probe screen. |  | Delete Probe This soft key deletes the current non-calibrated probe. Calibrated probes cannot be removed using this soft key.
| Apply or Confirm Changes This soft key accepts changes made to any fields, settings, or selections on the current screen. In some cases, this soft key adds a command to the NC Gage part program. |  | Cancel This soft key is initially disabled on this screen.
| Execute This accesses the Program screen where you can execute the part program. |  | Help This soft key accesses the NC Gage help file.
| Return This soft key returns the view up one level to the previous screen. |  | Forward When enabled, this soft key scrolls forward to any additional soft keys available on the second page for this screen.