### Step 3: Creating a New Probe

The Create New Probe screen lets you define the type of probe you will be using to measure your part.

1. Access the Create New Probe screen by pressing the following sequence of soft keys from the main screen:

- Press the Probe soft key.

- Press the Select a Probe soft key.

- Press the Create a New Probe soft key. The Create New Probe screen then appears.

2. Use the screen to provide the needed information about your probe. Type your probe's nominal diameter, the pocket number holding the probe, the probe's name, and any special instructions.

3. When finished, press the Confirm to Save Changes soft key.

Available Navigation Bar Soft Keys on this Screen:

| Backward When enabled, this soft key scrolls back to any additional buttons available on the first page for this screen. |  | Cancel This soft key clears any information entered into the Nominal Diameter and Pocket Number fields.
| Apply or Confirm Changes This soft key accepts changes made to any fields, settings, or selections on the current screen. In some cases, this soft key adds a command to the NC Gage part program. |  | Help This soft key accesses the NC Gage help file.
| Return This soft key returns the view up one level to the previous screen. |  | Forward When enabled, this soft key scrolls forward to any additional soft keys available on the second page for this screen.