### Step 4: Selecting a Probe

The Select Probe screen lets you choose what probe should measure your part.

1. Press the Probe soft key from the Main screen.

2. Press the Select a Probe soft key to display the Select Probe screen.

3. Select the probe you want to use from the Select a Probe list using the Select a Probe soft key .

4. Press the Confirm and Append Current Command to End soft key to save the changes or press the Return soft key to return to the previous screen without saving.

NC Gage will insert the probe into the part program's tree view.

Available Navigation Bar Soft Keys on this Screen:

| Create a New Probe This soft key lets you create a new probe by accessing the Create New Probe screen. |  | Delete Probe This soft key deletes the current non-calibrated probe. Calibrated probes cannot be removed using this soft key.
| Edit Probe This soft key displays the Edit Probe screen where a new probe can be defined. |  | Cancel This soft key is initially disabled on this screen.
| Execute This accesses the Program screen where you can execute the part program. |  |