### Dimension Distance

1. Press the Measure soft key from the Main screen's Navigation Bar.

2. Press the Forward soft key until you get to the third page of soft keys.

3. Press the Distance soft key to display the Distance screen.

The Distance option, located on the third page of the feature menu, lets you report the distance between two point type features. The distance can be in a single axis direction (parallel to an axis) or in a two axes direction.

1. To report a distance, select the axis direction, select the appropriate work face, and then select the two features. Only the valid feature types will show up in the selection screen. The graphics in the upper left corner of the screen will update to provide a visual cue as to how the feature will be built. The nominal and measured data will update according to the feature inputs.

2. Press the Confirm soft key to add the command to the program.

Valid Point Type Features:

- Circle Bore

- Circle Boss

- Corner Inside

- Corner Outside

- Constructed Points

Available Navigation Bar Soft Keys on this Screen: