## Work Face Setup

The Work Face Setup screen lets you define the orientation of the Work Face
soft key found throughout the software. A work face is simply the side of the part that will be measured. This setup screen is helpful if the computer monitor displaying NC Gage is not always in a fixed position around the machine tool. Using this screen, you can customize the setup of the work face icon or select default work face configurations.

To setup the work face:

1. Press the Setup soft key from the main screen.

2. Press the Setup Work Face Orientation for Machine soft key to display the Work Face Setup screen.

3. Either select a default configuration or define your own custom configuration.

4. Once you have defined the work face, press the Confirm soft key . Then throughout the software, each time the Work Face soft key is pressed, the software will use the work face defined here.

5. Press the Confirm soft key to save any changes made. Press the Return soft key to return to the previous screen without saving.

Note: A left handed setup is allowed. NC Gage will inform you when you are using this non-standard setup.