### Angle Between

1. Press the Measure soft key from the Main screen's Navigation Bar.

2. Press the Forward soft key until you get to the third page of soft keys.

3. Press the Angle Between soft key to display the Angle Between screen.

The Angle Between option, found on the third page of the feature menu, lets you report the angle between two line type features.

To Report an Angle

Select the appropriate work face.

1. Select the two line type features. NC Gage will calculate the angle based on the direction of the features. If the supplement of an angle, mark the Supplement check box. Only the valid feature types will show up in the selection screen. The graphics in the upper left corner of the screen will update to provide a visual cue as to how the feature will be built. The nominal and measured data will update according to the feature inputs.

2. Press the Confirm soft key to add the command to the program.

Valid Line Type Features:

- Web

- Pocket

- Line

- Constructed Lines

Available Navigation Bar Soft Keys on this Screen: