### Construct Line

1. Select the Measure soft key from the Main screen's Navigation Bar.

2. Select the Forward soft key to get to the third page of soft keys.

3. Select the Construct Line soft key to display the Construct Line screen.

This screen lets you create a line between two point type features.

To Construct a Line Feature

1. Select the appropriate work face.

2. Select the two point type features. Only the valid feature types will show up in the selection screen. The graphics in the upper left corner of the screen will update to provide a visual cue as to how the feature will be built. The nominal and measured data will update according to the feature inputs.

3. Press the Confirm soft key to add the command to the program.

Valid Point Type Features:

- Circle Bore

- Circle Boss

- Corner Inside

- Corner Outside

- Constructed Points

Available Navigation Bar Soft Keys on this Screen: