### Construct Point

1. Press the Measure soft key from the Main screen's Navigation Bar.

2. Press the Forward soft key to get to the third page of soft keys.

3. Press the Construct a Point soft key to display the Construct Point screen.

This screen lets you create a point feature by doing one of the following:

- Constructing a point at the intersection of two selected line type features by selecting the Intersection radio Option button.

- Constructing a point by projecting a point type feature onto a line type feature by selecting the Projection radio Option button.

- Constructing a point midway between two selected point type features by selecting the Midpoint radio Option button.

To Construct a Point Feature

1. From the Option section, select the appropriate option button for the type of construction to be made.

2. Select the appropriate work face using the Select Measurement Face soft key in the bottom toolbar.

3. Select the two features. Only the valid feature types will show up in the selection screen. The graphics in the upper left corner of the screen will update to provide a visual cue as to how the feature will be built. The nominal and measured data will update according to the feature inputs.

4. Press the Confirm soft key to add the command to the program.

Valid Point Type Features: | Valid Line Type Features:

- Circle Bore

- Circle Boss

- Corner Inside

- Corner Outside

- Constructed Points

- Web

- Pocket

- Line

- Constructed Lines

Available Navigation Bar Soft Keys on this Screen: