#### Modifying Default Parameters

Select the Edit | Setup | Modify Default Parameters menu option to open the Modify Default Parameters dialog box where you can edit the Inspection Plan default parameters.

Modify Default Parameters

The PC-DMIS Planner Default (.ipd) file is used to define the parameters for PC-DMIS Planner within PC-DMIS. This file allows you to determine how to take hits from features within the Inspection Plan. Feature parameters are specified for Auto Features, Constructed Features, and Dimensions. The install includes these two files that you can use as starting points for creating your own default parameters files:

- Default.ipd - A general defaults file.

- VoidDetection.ipd - A general defaults file for using void detection.

You can also specify how you want to display comments and features. See "Creating and Modifying a PC-DMIS Planner Default (.ipd) file".

The PC-DMIS Planner Rules (.ipr) script is used to specify rules for how automatic processes are performed on the Inspection Plan. Rules can be modified for certain criteria. For example, the number of hits taken on a circle based upon the diameter of the circle and so forth. See PC-DMIS Planner Rules (.ipr) script".

Before importing an Inspection Plan from a PC-DMIS Planner .cad file or an .ip file, you need to set up these files to apply to imported Inspection Plans.

More:

Creating and Modifying a PC-DMIS Planner Default (.ipd) file

PC-DMIS Planner Rules (.ipr) script