## Adding Dimensions to Features

PC-DMIS Planner allows you create both basic and Feature Control Frame (FCF) dimensions for any feature in the Inspection Plan. The available dimension types are:

Icon | Description
| Datum
| Location
| True Position
| Distance
| Angle Between
| Concentricity
| Coaxiality
| Circularity
| Cylindricity
| Straightness
| Flatness
| Perpendicularity
| Parallelism
| Total Runout
| Circular Runout
| Surface Profile
| Line Profile
| Angularity
| Symmetry

The Location, Distance, and Angle dimensions do not use Feature Control Frames (FCF) to display their information. These are Basic dimensions. All other dimensions use FCFs.

More:

Creating a Location Dimension

Creating a Distance Dimension

Creating an Angle Dimension

Creating Feature Control Frame Dimensions