## Creating a Blade Scan Profile Command

To create a Blade Scan Profile command, do the following:

1. Select the Insert | Modules | Blade Scan Profile... menu option. The Blade Scan Profile dialog box appears:

Blade Scan Profile dialog box

2. Complete the items in the dialog box.

Item | Description
ID box | Enter the name of this Blade Scan Profile command.
CV Sections area | This area displays a list of the convex (CV) sections in the part program.
CC Sections area | This area displays a list of the concave (CC) sections in the part program.
OK button | Click this button to insert the Blade Scan Profile command in the Edit window.