PC-Dmis 2010 Object Library | Send comments on this topic. | See Object Hierarchy Chart
PCDSTARTFEATFLAGS Enumeration
See Also

Collapse All Expand All

# Members

Member | Value | Description
--- | --- | ---
PCD_NORM | 0 | For auto circles, cylinders, ellipses, and slots. Do not combine with PCD_PIN. Default.
PCD_RECT | 0 | Values are in rectangular coordinates. Should not be combined with PCD_POLR. Default.
PCD_UNBND | 0 | Unbound line. Should not be ored with PCD_BND. Default.
PCD_OUT | 0 | Outside circle, sphere, cone, or cylinder. Should not be used with PCD_IN. Default.
PCD_LENGTH | 0 | Cone reports its length as opposed to angle. Do not or with PCD_ANGLE. Default.
PCD__EXTERIOR | 0 | Exterior angle hit. Only used for auto angle hits. Do not or with PCD_INTERIOR. Default.
PCD_MEASURE_SURFACE | 0 | Sets measure order. For auto edge points only. Default.
PCD_TRIM | 0 | For auto edge points only. Should not be ored with PCD_HEM. Default.
PCD__TOP | 0 |
PCD__ZPLUS | 0 |
PCD__ZAXIS | 0 |
PCD__ZMINUS | 1 |
PCD__BOTTOM | 1 |
PCD__XPLUS | 2 |
PCD__LEFT | 2 |
PCD__XAXIS | 2 |
PCD__XMINUS | 3 |
PCD__RIGHT | 3 |
PCD__YPLUS | 4 |
PCD__FRONT | 4 |
PCD__YAXIS | 4 |
PCD__YMINUS | 5 |
PCD__BACK | 5 |
PCD__INTERIOR | 8 | Interior angle hit. Only used for auto angle hits. Should not be combined with PCD_EXTERIOR.
PCD_POLR | 64 | Values are reported in cylindrical coordinates. Should not be combined with PCD_RECT.
PCD_IN | 128 | Inside circle, sphere, cone, or cylinder. Should not be combined with PCD_OUT.
PCD_ANGLE | 256 | Cone reports its angle as opposed to length. Should not be combined with PCD_LENGTH.
PCD_BND | 512 | Bound line. Should not be combined with PCD_UNBND.
PCD_MEASURE_EDGE | 1024 | Sets measure order. For auto edge points only.
PCD_MEASURE_BOTH | 2048 | Sets measure order. For auto edge points only.
PCD_HEM | 4096 | For auto edge points only. Should not be ored with PCD_TRIM.
PCD_PIN | 8192 | For auto circles, cylinders, ellipses, and slots. Do not or with PCD_NORM.
PCD_READPOS | 16384 | Turn read position on. For auto circles, cylinders, ellipses, and slots. Defaults to off.
PCD_LINE_3D | 32768 | 3D line. Used only for best fit lines. Default is a 2D line.
PCD__RECALC_NOMS | 65536 | Indicates that the theoretical values should be recalculated based on the theoretical hit values.
PCD_AUTOMOVE | 131072 | Causes move points to be automatically generated for auto features.
PCD_FINDHOLE | 262144 | For Auto Circles. Automatic finding of holes.
PCD_MEASURE_WIDTH | 524288 | Flag for Auto Square Slots.

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.