PC-Dmis 2010 Object Library | Send comments on this topic. | See Object Hierarchy Chart
Tip Object Members
See Also Overview

Collapse All Expand All

# Public Methods

ResetMeasToTheo | Resets measured tip data back to theo values

# Public Properties

a | Read Only: Returns the tilt of the tip Returns the A angle of the tip.
b | Read Only: Returns the rotation of the tip Returns the B angle of the tip.
C | Read Only: Returns the C angle of the tip
Date | Read Only: Gets/Sets string representing date of the last calibration of the tip in the format mm/dd/yy Returns the PC-DMIS representation of the most recent calibration date of the tip.
diam | Read/Write: Gets/Sets the theoretical diameter of the tip Returns the diameter of the tip.
DMISLabel | Read/Write: Gets/Sets the tip's DMIS Label
ID | Read Only: Returns the ID of the tip Returns the ID string of the tip.
IJK | Read Only: Returns a point data object with the measured vector of the tip A PointData object that returns the vector along which the tip lies. Read-only.
MeasDiam | Read/Write: Gets/Sets the measured diameter of the tip
MeasThickness | Read Only: Returns the measured thickness of the the tip
MeasXYZ | Read/Write: Gets/Sets the measured XYZ data of the tip
Nickname | Read/Write: Gets/Sets the tip's nickname
Parent | Read Only: Returns the parent tips object Returns the Tips collection object that contains this tip.
PrbRdv | Read Only: Returns the PRBRDV value for an analog probe calibration
Selected | Read/Write: Determines whether tip is selected to be qualified Determines whether tip is selected for qualification.
StandardDeviation | Read Only: Returns the standard deviation of the measured sphere after tip qualification
Thickness | Read Only: Returns the theoretical thickness of the tip Returns the nominal thickness of the tip.
Time | Read Only: Gets/Sets string representing time of the last calibration of the tip in the format HH:MM:SS Returns the PC-DMIS representation of the most recent calibration time of the tip.
TipNum | Read Only: Returns the tip number of the tip Returns the tip number in the list of tips.
TipType | Read Only: Returns the tip type of the tip Returns the type of the tip.
WristOffset | Read/Write: Returns a point data object with the wrist offset of the tip Returns the wrist offset of the tip.
WristTipIJK | Read Only: Returns a point data object with the theoretical vector of the tip Returns the wrist tip vector of the tip.
XYZ | Read/Write: Gets/Sets the theoretical XYZ data of the tip Returns the location of the tip.

# See Also

Tip Overview

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.