PC-Dmis 2010 Object Library | Send comments on this topic. | See Object Hierarchy Chart
Calibrate Method
See Also

Collapse All Expand All

sphere
  Id of measured sphere used in calibration.

tool
  Id of tool object used in calibration.

Moved
  Toggle indicating whether first hit should be taken manually or not. Can be either PCD_NO or PCD_YES.

# Description

Creates a probe calibration command

# Syntax

Visual Basic

    Public Sub Calibrate( _
       ByVal sphere As String, _
       ByVal tool As String, _
       ByVal Moved As PCDYESNO _
    )

# Parameters

sphere
  Id of measured sphere used in calibration.
tool
  Id of tool object used in calibration.
Moved

  Value | Description
  --- | ---
  PCD_YES |
  PCD_NO |

  Toggle indicating whether first hit should be taken manually or not. Can be either PCD_NO or PCD_YES.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.