PC-Dmis 2010 Object Library | Send comments on this topic. | See Object Hierarchy Chart
PutFeatData Method
See Also

Collapse All Expand All

ID

buffer

dtype

XYZ

IJK

# Description

Puts feature data into the command specified by the ID

# Syntax

Visual Basic

    Public Sub PutFeatData( _
       ByVal ID As String, _
       ByVal buffer As FeatData, _
       ByVal dtype As PCDMEASTHEO, _
       ByVal XYZ As XYZTYPES, _
       ByVal IJK As IJKTYPES _
    )

# Parameters

ID
buffer
dtype

  Value | Description
  --- | ---
  PCD_THEO |
  PCD__MEAS |

XYZ

  Value | Description
  --- | ---
  PCD_CENTROID |
  PCD_BALLCENTER |
  PCD_STARTPOINT |
  PCD_ENDPOINT |
  PCD_MIDPOINT |

IJK

  Value | Description
  --- | ---
  PCD__VECTOR |
  PCD_SLOTVECTOR |
  PCD_SURFACEVECTOR |

# Remarks

Parameters, allowed values, and limitations are identical to those of GetFeatData. The data currently in buffer is stored in the feature identified by the ID string.

# See Also

OldBasic Object

© Wilcox Associates, Inc. All Rights Reserved.

© 2010 All Rights Reserved.